{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","30","","","34"]
["","","Värme","Superlåg","m³/min","32","","","34"]
["Ljudeffektsnivå","Värme","","","dBA","","","62","","62"]
["","Kyla","","","dBA","","","60","","60"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","cfm","1059","","","1200"]
["","","Värme","Superlåg","cfm","1130","","","1200"]
["Mått","Enhet","","Höjd","mm","550","550","550","550","550","550"]
["","","","Bredd","mm","765","765","765","765","765","765"]
["","","","Djup","mm","285","285","285","285","285","285"]
["Vikt","Enhet","","","kg","36","36","36","41","41","41"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","760","500","500","890","500","500"]
["","","Värme","Superlåg","varv/min","820","320","320","890","500","500"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","","46.0","-10","46.0"]
["","","","Max.","°CTT","46","","-10","46","-10"]
["","Värme","Omgivning","Min.","°CVT","-15","","-15","-15","-15.0"]
["","","","Max.","°CVT","18","","18.0","18","18.0"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","46","46","","48","48"]
["","","","Nom.","dBA","48","","","46"]
["","Värme","","Hög","dBA","","48","48","","50","50"]
["","","","Nom.","dBA","50","","","48"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Mängd","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","GWP","","","","675","675.0","675","675","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","20 (1)","20","20 (1)","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15.0","15","15","15","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Total rörledningslängd","System","Verklig","m","30","30","30","30","30","30"]
["Standardtillbehör","Installation manual","","","","Installation manual","1","1","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Anm:","","","","","","(1) - För ett rum","","","","(1) - För ett rum"]
["","","","","","","","(1) - För ett rum","","(1) - För ett rum"]
["","","","","","","","(2) - Se separat ritning för driftsområde","","(2) - Se separat ritning för driftsområde"]
["","","","","","","","(3) - Se separata ritningar för elektriska data","","(3) - Se separata ritningar för elektriska data"]
["","","","","","","","(4) - Innehåller fluorerande växthusgas","","(4) - Innehåller fluorerande växthusgas"]
["Standardtillbehör","Reducer assembly","","","","","","","1","1","1"]