{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["Mått","Enhet","","Höjd","mm","550","550"]
["","","","Bredd","mm","765","765"]
["","","","Djup","mm","285","285"]
["Vikt","Enhet","","","kg","41","41"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","500","500"]
["","","Värme","Superlåg","varv/min","500","500"]
["Compressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","48","48"]
["","Värme","","Hög","dBA","50","50"]
["Köldmedium","Typ","","","","R-32","R-32"]
["","Mängd","","","kg","1.15","1.15"]
["","Mängd","","","tCO2Eq","0.78","0.8"]
["","GWP","","","","675","675.0"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)"]
["","Nivåskillnad","IU - OU","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Total rörledningslängd","System","Verklig","m","30","30"]
["Standardtillbehör","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-230-240","220-230-240"]
["Anm:","","","","","(1) - För ett rum","(1) - Alla D-AHU professionella kan konstrueras efter dina behov. Välj din AHU på tools.daikinapplied.eu"]