{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Mått","Enhet","","Höjd","mm","550","550","734"]
["","","","Bredd","mm","765","765","958"]
["","","","Djup","mm","285","285","340"]
["Vikt","Enhet","","","kg","36","41","60"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min (2)","500","500","420"]
["","","Värme","Superlåg","varv/min (2)","320","500","420"]
["Compressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","","-10"]
["","","","Max.","°CTT","","","46"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Värme","","Hög","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","Mängd","","","kg","0.88","1.15","2"]
["","Mängd","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","25"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","15.0","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Total rörledningslängd","System","Verklig","m","30","30","50"]
["Standardtillbehör","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-230-240","220-230-240","220-240"]
["Anm:","","","","","(1) - För ett rum","(1) - För ett rum","(1) - För ett rum"]
["Standardtillbehör","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]