{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","48","48","","50","50"]
["","Kyla","","Nom.","dBA","47","47","","48","48"]
["Standardtillbehör","Installationsanvisning","","","","1","1","","1","1"]
["","Skruvpåse","","","","1","1","","1","1"]
["","Kondensvattenplugg","","","","1","1","","1","1"]
["Köldmedium","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Mängd","","","kg","1.20","1.20","","1.60","1.60"]
["","Typ","","","","R-410A","R-410A","","R-410A","R-410A"]
["Röranslutningar","Nivåskillnad","IU - IU","Max.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Max.","m","15","15","","15","15"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)","","0,02 (för rördragning över 20m)","0,02 (för rördragning över 20m)"]
["","Total rörledningslängd","System","Verklig","m","30","30","","30","30"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","765","765","","765","765"]
["","","","Djup","mm","285","285","","285","285"]
["","","","Höjd","mm","550","550","","550","550"]
["Vikt","Enhet","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frequency","","","Hz","50","50","","50","50"]
["","Spänning","","","V","220-240","220-240","","220-240","220-240"]
["Anm:","","","","","(1) - Innehåller fluorerande växthusgas","(1) - Innehåller fluorerande växthusgas","","(1) - Innehåller fluorerande växthusgas","(1) - Innehåller fluorerande växthusgas"]
["Mått","Enhet","","Höjd","mm","","","550","","","550"]
["","","","Bredd","mm","","","765","","","765"]
["","","","Djup","mm","","","285","","","285"]
["Vikt","Enhet","","","kg","","","38","","","42"]
["Kompressor","Type","","","","","","Hermetiskt tillsluten swing-kompressor","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","","10","","","10"]
["","","","Max.","°CTT","","","46","","","46"]
["","Värme","Omgivning","Min.","°CVT","","","-15","","","-15"]
["","","","Max.","°CVT","","","15.5","","","15.5"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","","","47","","","48"]
["","Värme","","Nom.","dBA","","","48","","","50"]
["Köldmedium","Typ","","","","","","R-410A","","","R-410A"]
["","Mängd","","","kg","","","1.20","","","1.60"]
["","Mängd","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","","20","","","20"]
["","Extra köldmediemängd","","","kg/m","","","0,02 (för rördragning över 20m)","","","0,02 (för rördragning över 20m)"]
["","Nivåskillnad","IU - OU","Max.","m","","","15","","","15"]
["","","IU - IU","Max.","m","","","7.5","","","7.5"]
["","Total rörledningslängd","System","Verklig","m","","","30","","","30"]
["Standardtillbehör","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Strömförsörjning","Fas","","","","","","1~","","","1~"]
["","Frequency","","","Hz","","","50","","","50"]
["","Spänning","","","V","","","220-240","","","220-240"]
["Standardtillbehör","Reducerare","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]