{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","47"]
["","Kyla","","Nom.","dBA","46"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Skruvpåse","","","","1"]
["","Kondensvattenplugg","","","","1"]
["","Kondensvattenplugg (1)","","","","6"]
["","Kondensvattenplugg (2)","","","","3"]
["","Avtagbar F-gas-etikett","","","","1"]
["","Extra köldmediaetikett","","","","1"]
["Köldmedium","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Mängd","","","kg","1.8"]
["","Typ","","","","R-32"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","420"]
["","","Värme","Superlåg","varv/min","420"]
["Röranslutningar","Nivåskillnad","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)"]
["","Total rörledningslängd","System","Verklig","m","50"]
["Compressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","868"]
["","","","Djup","mm","320"]
["","","","Höjd","mm","734"]
["Vikt","Enhet","","","kg","57"]
["Power supply","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Innehåller fluorerande växthusgas"]
["","","","","","(2) - Se separat ritning för driftsområde"]
["","","","","","(3) - Se separata ritningar för elektriska data"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","","24"]
["","","Värme","Superlåg","m³/min","","24"]
["","","","Superlåg","cfm","","847"]
["","","Värme","Superlåg","cfm","","847"]
["Mått","Enhet","","Höjd","mm","","734"]
["","","","Bredd","mm","","868"]
["","","","Djup","mm","","320"]
["Vikt","Enhet","","","kg","","57"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","","420"]
["","","Värme","Superlåg","varv/min","","420"]
["Compressor","Typ","","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","-10"]
["","","","Max.","°CTT","","46"]
["","Värme","Omgivning","Min.","°CVT","","-15"]
["","","","Max.","°CVT","","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","","46"]
["","Värme","","Nom.","dBA","","47"]
["Köldmedium","Typ","","","","","R-32"]
["","Mängd","","","kg","","1.80"]
["","Mängd","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","25"]
["","Extra köldmediemängd","","","kg/m","","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","","15"]
["","","IU - IU","Max.","m","","7.5"]
["","Total rörledningslängd","System","Verklig","m","","50"]
["Standardtillbehör","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Strömförsörjning","Fas","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","220-240"]