{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-A8"]
[]
[]
[]
[]
["","","","","","3MXM40A2V1B8","3MXM52A2V1B8","3MXM68A2V1B8"]
["Mått","Enhet","","Höjd","mm","734","734","734"]
["","","","Bredd","mm","974","974","974"]
["","","","Djup","mm","408","408","408"]
["Vikt","Enhet","","","kg","57","57","62"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","-10","-10"]
["","","","Max.","°CTT","50","50","50"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46","46","48"]
["","Värme","","Nom.","dBA","47","47","48"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","Mängd","","","kg","1.80","1.80","2.00"]
["","Mängd","","","tCO2Eq","1.22","1.22","1.35"]
["","GWP","","","","675","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","25 (1)","25 (1)","25 (1)"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)","0,02 (för rördragning över 30m)","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Total rörledningslängd","System","Verklig","m","50 (2)","50 (2)","50"]
["Standardtillbehör","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240"]
["Anm:","","","","","(1) - För ett rum","(1) - För ett rum","(1) - För ett rum"]
["","","","","","(2) - För kombination med CVXM-A, FVXM-A - maximal rörledningslängd är 30 m.","(2) - För kombination med CVXM-A, FVXM-A - maximal rörledningslängd är 30 m.","(2) - För kombination med CVXM-A, FVXM-A - maximal rörledningslängd är 30 m."]
["","","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]
["","","","","","(5) - Innehåller fluorerande växthusgas","(5) - Innehåller fluorerande växthusgas","(5) - Innehåller fluorerande växthusgas"]
["Standardtillbehör","FTXJ42A2V1BS","","","","","FTXJ42A2V1BS"]
["","FVXM25B2V1B","","","","","","FVXM25B2V1B"]