{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B (Archived)","4MXM80N2V1B (Archived)"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","24.1","24.1"]
["","","Värme","Superlåg","m³/min","24.1","24.1"]
["","","","Superlåg","cfm","851","851.0"]
["","","Värme","Superlåg","cfm","851.0","851.0"]
["Mått","Enhet","","Höjd","mm","734","734"]
["","","","Bredd","mm","958","958"]
["","","","Djup","mm","340","340"]
["Vikt","Enhet","","","kg","63","67"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","-10"]
["","","","Max.","°CTT","46","46"]
["","Värme","Omgivning","Min.","°CVT","-15","-15"]
["","","","Max.","°CVT","18","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","48","49"]
["","Värme","","Nom.","dBA","48","49"]
["Köldmedium","Typ","","","","R-32","R-32"]
["","Mängd","","","kg","2.00","2.40"]
["","Mängd","","","tCO2Eq","1.4","1.6"]
["","GWP","","","","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","25","25"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Total rörledningslängd","System","Verklig","m","60","70"]
["Standardtillbehör","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-240","220-240"]