{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Mått","Enhet","","Höjd","mm","734","734"]
["","","","Bredd","mm","1,040","1,040"]
["","","","Djup","mm","408","408"]
["Vikt","Enhet","","","kg","69","73"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","48","52"]
["","Värme","","Nom.","dBA","49","53"]
["Köldmedium","Typ","","","","R-32","R-32"]
["","Mängd","","","kg","2","2.4"]
["","Mängd","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","25 (2)","25 (3)"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","15 (3)","15"]
["","","IU - IU","Max.","m","7.5 (3)","7.5 (3)"]
["","Total rörledningslängd","System","Verklig","m","60","75"]
["Standardtillbehör","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-440","220-240"]
["Anm:","","","","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","","(2) - För ett rum","(2) - För ett rum"]
["","","","","","(3) - För ett rum (för kombination med FBA71/100/125 och EKHWET och CKHWS, se installationsanvisningar)","(3) - För ett rum (för kombination med FBA71/100/125 och EKHWET och CKHWS, se installationsanvisningar)"]
["","","","","","(4) - Innehåller fluorerande växthusgas","(4) - Innehåller fluorerande växthusgas"]