{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A9"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B9"]
["Mått","Enhet","","Höjd","mm","734"]
["","","","Bredd","mm","974"]
["","","","Djup","mm","408"]
["Vikt","Enhet","","","kg","68"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10"]
["","","","Max.","°CTT","46"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","52"]
["","Värme","","Nom.","dBA","52"]
["Köldmedium","Typ","","","","R-32"]
["","Mängd","","","kg","2.4"]
["","Mängd","","","tCO2Eq","1.62"]
["","GWP","","","","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","25 (1)"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Total rörledningslängd","System","Verklig","m","75"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Kondensvattenplugg","","","","1"]
["","Reducerare","","","","1"]
["","Skruvpåse","","","","1"]
["Intervall för energieffektivitet","","","","","A+++ ~ D"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - För ett rum"]
["","","","","","(2) - För kombination med CVXM-A, FVXM-A - maximal rörledningslängd är 30 m."]
["","","","","","(3) - Se separat ritning för driftsområde"]
["","","","","","(4) - Se separata ritningar för elektriska data"]
["","","","","","(5) - Innehåller fluorerande växthusgas"]