{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXS-E"]
[]
[]
[]
[]
["","","","","","5MXS90E3V3B2","5MXS90E3V3B","5MXS90E7V3B"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","52","52"]
["","Kyla","","Nom.","dBA","52","52"]
["Standardtillbehör","Installationsanvisning","","","","1","1"]
["","Kondensvattenplugg","","","","1","1"]
["","Reducerare","","","","1","1"]
["Köldmedium","Charge","","","TCO2Eq","6.2","6.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Mängd","","","kg","2.99","2.99"]
["","Typ","","","","R-410A","R-410A"]
["Driftsområde","Kyla","Omgivning","Max.","°CTT","46"]
["","","","Min.","°CTT","-10"]
["","Värme","Omgivning","Max.","°CVT","18"]
["","","","Min.","°CVT","-15"]
["Röranslutningar","Nivåskillnad","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)"]
["","Total rörledningslängd","System","Verklig","m","75"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhets-","","Bredd","mm","900","900"]
["","","","Djup","mm","320","320"]
["","","","Höjd","mm","770","770"]
["Vikt","Enhet","","","kg","73","73"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","230","230"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 7,5m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 7,5m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7.5m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7.5m"]
["","","","","","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas"]
["Röranslutningar","Nivåskillnad","IU - IU","Max.","m","","7.5"]
["","","IU - OU","Max.","m","","15"]
["","Extra köldmediemängd","","","kg/m","","0,02 (för rördragning över 30m)"]
["","Total rörledningslängd","System","Verklig","m","","75"]
["Kompressor","Type","","","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Höjd","mm","","","770"]
["","","","Bredd","mm","","","900"]
["","","","Djup","mm","","","320"]
["Vikt","Enhet","","","kg","","","73"]
["Kompressor","Type","","","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","","-10"]
["","","","Max.","°CTT","","","46"]
["","Värme","Omgivning","Min.","°CVT","","","-15"]
["","","","Max.","°CVT","","","15.5"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","","","52"]
["","Värme","","Nom.","dBA","","","52"]
["Köldmedium","Typ","","","","","","R-410A"]
["","Mängd","","","kg","","","2.99"]
["","Mängd","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","","25"]
["","Extra köldmediemängd","","","kg/m","","","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Total rörledningslängd","System","Verklig","m","","","75"]
["Standardtillbehör","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Strömförsörjning","Fas","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Spänning","","","V","","","230"]