{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Kylkapacitet","Nom.","","kW","9.5","12.1 (1)"]
["Rumskyla","SEER","","","4.65","4.68"]
["","Årlig energiförbrukning","","kWh/a","716","1,550"]
["","Kapacitet","Pdesign","kW","9.50","12.1"]
["","Energieffektivitetsklass","","","B"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Energieffektivitetsklass","","","A"]
["","Årlig energiförbrukning","","kWh/a","2,498","3,340"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","1,813"]
["","EER köldfaktor","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Energimärkningsdirektiv","Kyla","","D"]
["","","Värme","","B"]
["Värmekapacitet","Nom.","","kW","10.8","13.5 (2)"]
["Anm:","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 7,5 m, nivåskillnad: 0 m"]
["","","","","(2) - Årlig energiförbruking enligt Energimärkningsdirektiv 2002/31/EC","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7,5 m, nivåskillnad: 0 m"]
["","","","","(3) - SEER och SCOP är enligt EN 14825","(3) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","(4) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]