{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardtillbehör","Installationsanvisning","","","","Installationsanvisning"]
["","Bruksanvisning","","","","Bruksanvisning"]
["","Skruv + bricka","","","","Skruv + bricka"]
["","Trådlös fjärrkontroll","","","","Trådlös fjärrkontroll"]
["","Täcklocksgaller","","","","Täcklocksgaller"]
["","Batteri","","","","Batteri"]
["Röranslutningar","Vätska","","YD","mm","9.52"]
["","Gas","","YD","mm","15.88"]
["","Kondensvatten","","","","19.05"]
["Ineffekt","Kyla","","Nom.","kW","0.128"]
["","Värme","","Nom.","kW","0.128"]
["Ljudeffektsnivå","Kyla","","","dBA","64"]
["","Värme","","","dBA","64"]
["Mått","Enhet","","Bredd","mm","600"]
["","","","Djup","mm","1,007"]
["","","","Höjd","mm","285"]
["Hölje","Material","","","","Galvaniserat stål"]
["Vikt","Enhet","","","kg","35"]
["Fläkt","Yttre statiskt tryck","","Hög","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Låg","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Namn","","","","V1"]
["","Spänning","","","V","220-240"]
["Ineffekt","Värme","","Nom.","kW","","0.109"]
["","Kyla","","Nom.","kW","","0.109"]
["Fläkt","Yttre statiskt tryck","","Hög","Pa","","70","150","150"]
["","","","Låg","Pa","","45","111","92"]
["Hölje","Material","","","","","Galvaniserat stål"]
["Mått","Enhet","","Höjd","mm","","378","378","378"]
["","","","Bredd","mm","","541","1300","1500"]
["","","","Djup","mm","","1045","541","541"]
["Vikt","Enhet","","","kg","","44","50","56"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Låg","m³/min","","18.3","34.8","37.9"]
["","","Värme","Hög","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Låg","m³/min","","18.3","34.8","37.9"]
["","Yttre statiskt tryck","","Nom.","Pa","","57","128","122"]
["Ljudeffektsnivå","Kyla","","","dBA","","60","72","73"]
["","Värme","","","dBA","","60","72","73"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Låg","dBA","","36","50","50"]
["","Värme","","Hög","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Låg","dBA","","36","50","50"]
["Röranslutningar","Vätska","","YD","mm","","9.52","9.52","9.52"]
["","Gas","","YD","mm","","15.88","15.9","15.9"]
["","Kondensvatten","","","","","19.05"]
["Standardtillbehör","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Strömförsörjning","Fas","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","220-240"]
["Kylkapacitet","Total kapacitet","","Nom.","kW","","","12.10","13.00"]
["Värmekapacitet","Total kapacitet","","Nom.","kW","","","13.5","15.5"]
["Hölje","Färg","","","","","","Galvaniserad stålplåt / omålad","Galvaniserad stålplåt / omålad"]
["Fläkt","Luftflödeshastighet","Kyla","Medel","m³/min","","","37","44"]
["","","Värme","Medel","m³/min","","","37.4","43.9"]
["Ljudtrycksnivå","Kyla","","Medel","dBA","","","52","53"]
["","Värme","","Medel","dBA","","","52","53"]
["Styrsystem","Infraröd fjärrkontroll","","","","","","ARCWLA","ARCWLA"]