{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A"]
[]
[]
[]
[]
["","","","","ADEA50A2VEB / ARXM50A5V1B","ADEA60A2VEB / ARXM60A5V1B","ADEA71A2VEB / ARXM71A5V1B"]
["Kylkapacitet","Nom.","","kW","5.00","5.7","6.8"]
["","Max.","","kW","","","6.98"]
["Värmekapacitet","Nom.","","kW","5.50","7","7.5"]
["","Max.","","kW","","","7.66"]
["Nominell verkningsgrad","EER köldfaktor","","","3.27","3.43","2.95"]
["","COP","","","3.74","3.63","3.49"]
["","Årlig energiförbrukning","","kWh","765","831","1153"]
["","Energimärkningsdirektiv","Kyla","","A","A","C"]
["","","Värme","","A","A","B"]
["Rumskyla","Energieffektivitetsklass","","","A+","A+","A"]
["","Kapacitet","Pdesign","kW","5.00","5.7","6.8"]
["","SEER","","","5.65","5.74","5.35"]
["","Årlig energiförbrukning","","kWh/a","310","347","445"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A+","A+","A"]
["","Kapacitet","Pdesign","kW","4.40","4.6","6"]
["","SCOP/A","","","4.00","4","3.8"]
["","Pdh Värmekapacitet vid -10°","","kW","3.73","4","4.83"]
["","Årlig energiförbrukning","","kWh/a","1538","1610","2209"]
["Anm:","","","","","(1) - Se separat ritning för driftsområde","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","","(2) - Se separata ritningar för elektriska data","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","","(3) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(3) - Se separat ritning för driftsområde"]
["","","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(4) - Se separata ritningar för elektriska data"]