{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":11,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Ljudtrycksnivå","Värme","","Hög","dBA","37","37","31"]
["","","","Medel","dBA","34","34","28"]
["","","","Låg","dBA","29","29","25"]
["","Kyla","","Medium","dBA","32","32","28"]
["","","","Låg","dBA","29","29","25"]
["","","","Hög","dBA","35","35","30"]
["Standardtillbehör","Bruksanvisning","","","","1","1","1"]
["","Installationsanvisning","","","","1","1","1"]
["","Kondensvattenslang","","","","1","1","1"]
["","Metallklämma för kondensvattenslang","","","","1","1","1"]
["","Bricka för hängarfäste","","","","8","8","8"]
["","Skruvar","","","","40","40","40"]
["","Isolering för anslutningsdel","","","","2","2","2"]
["","Tätningsbelägg","","","","5","5","5"]
["","Rörhållare","","","","4","4","4"]
["Styrsystem","Wired remote control","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35","6.35"]
["","Gas","","YD","mm","9.52","12.70","12.70"]
["","Kondensvatten","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Kyla","","","dBA","60","60","56"]
["Mått","Enhet","","Bredd","mm","700","700","1,000"]
["","","","Djup","mm","800","800","800"]
["","","","Höjd","mm","245","245","245"]
["Hölje","Material","","","","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt"]
["","Färg","","","","Ej lackerad (galvaniserad)","Ej lackerad (galvaniserad)","Ej lackerad (galvaniserad)"]
["Vikt","Enhet","","","kg","28.0","28.0","35.0"]
["Fläkt","Yttre statiskt tryck","","Hög","Pa","150","150","150"]
["","","","Nom.","Pa","30","30","30"]
["","Luftflödeshastighet","Värme","Hög","m³/min","15.0","15.0","18.0"]
["","","","Låg","m³/min","10.5","10.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0"]
["","","Kyla","Låg","m³/min","10.5","10.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0"]
["","","","Hög","m³/min","15.0","15.0","18.0"]
["Dräneringshöjd","mm","","","","625","625","625"]
["Power supply","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-240/220","220-240/220","220-240/220"]
["Anm:","","","","","(1) - Ljudeffektsnivån är ett absolutvärde för vad en ljudkälla ger upphov till.","(1) - Ljudeffektsnivån är ett absolutvärde för vad en ljudkälla ger upphov till.","(1) - Ljudeffektsnivån är ett absolutvärde för vad en ljudkälla ger upphov till.","(1) - Ljudeffektsnivån är ett absolutvärde för vad en ljudkälla ger upphov till.","(1) - Ljudeffektsnivån är ett absolutvärde för vad en ljudkälla ger upphov till.","(1) - Ljudeffektsnivån är ett absolutvärde för vad en ljudkälla ger upphov till."]
["","","","","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["Fläkt","Yttre statiskt tryck","","Hög","Pa","","","","150","150","150"]
["Hölje","Färg","","","","","","","Ej lackerad (galvaniserad)","Ej lackerad (galvaniserad)","Ej lackerad (galvaniserad)"]
["","Material","","","","","","","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt"]
["Mått","Enhet","","Höjd","mm","","","","245","245","245"]
["","","","Bredd","mm","","","","1000","1400","1400"]
["","","","Djup","mm","","","","800","800","800"]
["Vikt","Enhet","","","kg","","","","35","46","46"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","","","18","29","34"]
["","","","Medel","m³/min","","","","15","26","29"]
["","","","Låg","m³/min","","","","12.5","23","23.5"]
["","","Värme","Hög","m³/min","","","","18","29","34"]
["","","","Medel","m³/min","","","","15","26","29"]
["","","","Låg","m³/min","","","","12.5","23","23.5"]
["","Yttre statiskt tryck","","Nom.","Pa","","","","30","40","50"]
["Ljudeffektsnivå","Kyla","","","dBA","","","","56","58","62"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","","","30","34","37"]
["","","","Medel","dBA","","","","28","32","35"]
["","","","Låg","dBA","","","","25","30","32"]
["","Värme","","Hög","dBA","","","","31","36","38"]
["","","","Medel","dBA","","","","28","33","35"]
["","","","Låg","dBA","","","","25","30","32"]
["Röranslutningar","Vätska","","YD","mm","","","","9.52","9.52","9.52"]
["","Gas","","YD","mm","","","","15.9","15.9","15.9"]
["","Kondensvatten","","","","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Dräneringshöjd","mm","","","","","","","625","625","625"]
["Styrsystem","Infraröd fjärrkontroll","","","","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Kabelansluten fjärrkontroll","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardtillbehör","Installation manual","","","","","","","1","1","1"]
["","Washer for hanger bracket","","","","","","","8","8","8"]
["","Operation manual","","","","","","","1","1","1"]
["","Clamps","","","","","","","4","4","4"]
["","Drain hose","","","","","","","1","1","1"]
["","Insulation for fitting","","","","","","","2","2","2"]
["","Metal clamp for drain hose","","","","","","","1","1","1"]
["","Screws","","","","","","","40","40","40"]
["","Sealing pads","","","","","","","5","5","5"]
["Strömförsörjning","Fas","","","","","","","1~","1~","1~"]
["","Frequency","","","Hz","","","","50","50","50"]
["","Spänning","","","V","","","","220-240/220","220-240/220","220-240/220"]
["Kylkapacitet","Total kapacitet","","Nom.","kW","","","","","","14.00"]
["Värmekapacitet","Total kapacitet","","Nom.","kW","","","","","","13.50"]