{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEQ71C2VEB / AZQS71B2V1B","ADEQ100C2VEB / AZQS100B8V1B","ADEQ125C2VEB / AZQS125B8V1B"]
["Kylkapacitet","Nom.","","kW","","9.50 (1)","12.1 (1)"]
["Rumskyla","SEER","","","","5.10","4.71"]
["","Årlig energiförbrukning","","kWh/a","","652","1,543"]
["","Kapacitet","Pdesign","kW","","9.50","12.1"]
["","Energieffektivitetsklass","","","","A"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","","7.60","7.93"]
["","SCOP/A","","","","3.81","3.50"]
["","Energieffektivitetsklass","","","","A"]
["","Årlig energiförbrukning","","kWh/a","","2,793","3,167"]
["Nominell verkningsgrad","EER köldfaktor","","","","","2.27"]
["Värmekapacitet","Nom.","","kW","","10.8 (2)","13.5 (2)"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 7,5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 7,5 m, nivåskillnad: 0 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7,5 m, nivåskillnad: 0 m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 7,5 m, nivåskillnad: 0 m"]
["Intervall för energieffektivitet","","","","A+++ ~ D"]