{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Ljudtrycksnivå","Värme","Hög","dBA","37","37","31","31","36","38"]
["","","Nom.","dBA","37","37","31","31","36","38"]
["","","Medel","dBA","34","34","28","28","33","35"]
["","","Låg","dBA","29","29","25","25","30","32"]
["","Kyla","Medium","dBA","32","32","28","28","32","35"]
["","","Låg","dBA","29","29","25","25","30","32"]
["","","Hög","dBA","35","35","30","30","34","37"]
["","","Nom.","dBA","35","35","30","30","34","37"]
["Standardtillbehör","Bruksanvisning","","","1","1","1","1","1","1"]
["","Installationsanvisning","","","1","1","1","1","1","1"]
["","Kondensvattenslang","","","1","1","1","1","1","1"]
["","Metallklämma för kondensvattenslang","","","1","1","1","1","1","1"]
["","Bricka för hängarfäste","","","8","8","8","8","8","8"]
["","Skruvar","","","40","40","40","40","40","40"]
["","Isolering för anslutningsdel","","","2","2","2","2","2","2"]
["","Tätningsbelägg","","","5","5","5","5","5","5"]
["","Rörhållare","","","4","4","4","4","4","4"]
["Köldmedium","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Kylkapacitet","Total kapacitet","Nom.","kW","","","","","","12.10"]
["Röranslutningar","Vätska","YD","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gas","YD","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Kondensvatten","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Kyla","","dBA","60","60","56","56","58","62"]
["Mått","Enhet","Bredd","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Djup","mm","800","800","800","800","800","800"]
["","","Höjd","mm","245","245","245","245","245","245"]
["Hölje","Material","","","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt","Galvaniserad stålplåt"]
["","Färg","","","Omålat","Omålat","Omålat","Omålat","Omålat","Omålat"]
["Vikt","Enhet","","kg","28.0","28.0","35.0","35","46","46"]
["Fläkt","Yttre statiskt tryck","Hög","Pa","150","150","150","150","150","150"]
["","","Nom.","Pa","30","30","30","30","40","50"]
["Värmekapacitet","Total capacity","Nom.","kW","","","","","","13.5"]
["Power supply","Fas","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50","50","50"]
["","Spänning","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Anm:","","","","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(1) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar."]