{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-N9"]
[]
[]
[]
[]
["","","","","","ARXM25N2V1B9","ARXM25N5V1B9","ARXM35N5V1B9","ARXM35N2V1B9","ARXM50N2V1B9","ARXM60N2V1B9","ARXM71N2V1B9"]
["Mått","Enhet","","Höjd","mm","550","550","550","550","734","734","734"]
["","","","Bredd","mm","765","765","765","765","870","870","870"]
["","","","Djup","mm","285","285","285","285","373","373","373"]
["Vikt","Enhet","","","kg","32","32","32","32","50","50.0","50.0"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","-10","-10","","-10","-10","-10"]
["","","","Max.","°CTT","","50","50","","50","46","46"]
["","Värme","Omgivning","Min.","°CVT","","-21","-21","","-21","-15","-15"]
["","","","Max.","°CVT","","18","18","","18","18","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46","46","49","49","48","48","52"]
["","Värme","","Nom.","dBA","47","47","49","49","49","49","52"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","0.76","0.76","0.76","0.76","1.15","1.15","1.15"]
["","Mängd","","","tCO2Eq","0.52","0.52","0.52","0.52","0.78","0.78","0.78"]
["","GWP","","","","675","675","675","675","675","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","20","20","30","30","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,020 (för rördragning över 10 m)","0,035 (för rördragning över 10 m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15","15","15","20","20","20"]
["Standardtillbehör","Installation manual","","","","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardtillbehör","Drain cap","","","","","","","","3","3","3"]
["Kompressor","Typ","","","","","","","","","","Hermetiskt tillsluten swing-kompressor"]