{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","","49.0"]
["","Kyla","","Nom.","dBA","","49.0"]
["Standardtillbehör","Kondensvattenplugg","","","","","1"]
["","Installationsanvisning","","","","","1"]
["","Etikett för köldmediemängd","","","","","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","","1"]
["","Allmänna säkerhetsföreskrifter","","","","","1"]
["Köldmedium","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Mängd","","","kg","","0.76"]
["","Typ","","","","","R-32"]
["Driftsområde","Kyla","Omgivning","Max.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","","15"]
["","Extra köldmediemängd","","","kg/m","","0,02 (för rördragning över 10m)"]
["Compressor","Typ","","","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","","840"]
["","","","Djup","mm","","350"]
["","","","Höjd","mm","","552"]
["Vikt","Enhet","","","kg","","32"]
["Power supply","Fas","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","220-240"]
["Anm:","","","","","(1) - Endast möjlig i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Innehåller fluorerande växthusgas"]
["","","","","","(2) - Endast möjlig i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Se separat ritning för driftsområde"]
["","","","","","","(3) - Se separata ritningar för elektriska data"]
["","","","","","","(4) - Endast möjlig i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Endast möjlig i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Mått","Enhet","","Höjd","mm","552"]
["","","","Bredd","mm","840"]
["","","","Djup","mm","350"]
["Vikt","Enhet","","","kg","32"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","-10"]
["","","","Max.","°CDB","50 (4), 46 (5)"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46.0"]
["","Värme","","Nom.","dBA","47.0"]
["Köldmedium","Mängd","","","kg","0.76"]
["","Mängd","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","15"]
["Standardtillbehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Strömförsörjning","Frequency","","","Hz","50"]