{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Ljudtrycksnivå","Värme","","Hög","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Kyla","","Hög","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standardtillbehör","Kondensvattenplugg","","","","","1","1","1","1"]
["","Installationsanvisning","","","","","1","1","1","1"]
["","Etikett för köldmediemängd","","","","","1","1","","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","","1","1","","1"]
["Köldmedium","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Mängd","","","kg","","1.70","1.0","1.2","1.50"]
["","Typ","","","","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Varvtal","Kyla","Superlåg","varv/min","","","780","780"]
["","","Värme","Superlåg","varv/min","","","740","740"]
["Driftsområde","Kyla","Omgivning","Max.","°CTT","","46","46","46","46"]
["","","","Min.","°CTT","","-10","10","10","-10"]
["","Värme","Omgivning","Max.","°CVT","","18","18","18","18"]
["","","","Min.","°CVT","","-15","-15","-15","-15"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","","20.0","15","15","20.0"]
["","Extra köldmediemängd","","","kg/m","","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["Ljudeffektsnivå","Kyla","","","dBA","","65","","","62"]
["","Värme","","","dBA","","65","","","62"]
["Compressor","Typ","","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","","825","765","765","825"]
["","","","Djup","mm","","300","285","285","300"]
["","","","Höjd","mm","","735","550","550","735"]
["Vikt","Enhet","","","kg","","47","34","34","47"]
["Fläkt","Luftflöde","Värme","Superlåg","cfm","","","904","904"]
["","","","Superlåg","m³/min","","","25.6","25.6"]
["","","Kyla","Superlåg","m³/min","","","30.1","30.1"]
["","","","Superlåg","cfm","","","1,063","1,063"]
["Power supply","Fas","","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50","50"]
["","Spänning","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Anm:","","","","","(1) - 220V","","(1) - Vid anslutning till en utomhusdel med multisystem, se specifikationerna för multiutomhusdelen som ska anslutas.","(1) - Vid anslutning till en utomhusdel med multisystem, se specifikationerna för multiutomhusdelen som ska anslutas."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Innehåller fluorerande växthusgas","(5) - Innehåller fluorerande växthusgas"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","48.9"]
["","","Värme","Superlåg","m³/min","43.1"]
["","","","Superlåg","cfm","1727"]
["","","Värme","Superlåg","cfm","1522"]
["Mått","Enhet","","Höjd","mm","735"]
["","","","Bredd","mm","825"]
["","","","Djup","mm","300"]
["Vikt","Enhet","","","kg","47"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","670"]
["","","Värme","Superlåg","varv/min","670"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","10"]
["","","","Max.","°CTT","46"]
["","Värme","Omgivning","Min.","°CVT","-15"]
["","","","Max.","°CVT","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","48"]
["","Värme","","Hög","dBA","48"]
["Köldmedium","Typ","","","","R-410A"]
["","Mängd","","","kg","1.7"]
["","Mängd","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","20"]
["Standardtillbehör","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","","(1) - Innehåller fluorerande växthusgas","","","(1) - Innehåller fluorerande växthusgas"]