{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","","48"]
["","","","Låg","dBA","","45"]
["Standardtillbehör","1","","","","","550"]
["Köldmedium","Mängd","","","kg","","2.5"]
["","Typ","","","","","1.2"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","","30.1"]
["","","","Superlåg","cfm","","1,063"]
["Fläktmotor","Varvtal","Kyla","Superlåg","varv/min","","740"]
["","","Värme","Superlåg","varv/min","","-15"]
["Driftsområde","Värme","Omgivning","Min.","°CVT","","20"]
["","","","Max.","°CVT","","10"]
["Ljudtrycksnivå","Kyla","","Låg","dBA","","44"]
["","","","Hög","dBA","","48"]
["Compressor","Typ","","","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","","285"]
["","","","Djup","mm","","612"]
["","","","Höjd","mm","","765"]
["Vikt","Enhet","","","kg","","34"]
["Fläkt","Luftflödeshastighet","Värme","Superlåg","cfm","","904"]
["","","","Superlåg","m³/min","","25.6"]
["Power supply","Fas","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","220-240"]
["Anm:","","","","","(1) - 220V","(1) - Innehåller fluorerande växthusgas"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","30.1"]
["","","Värme","Superlåg","m³/min","25.6"]
["","","","Superlåg","cfm","1063"]
["","","Värme","Superlåg","cfm","904"]
["Mått","Enhet","","Höjd","mm","550"]
["","","","Bredd","mm","765"]
["","","","Djup","mm","285"]
["Vikt","Enhet","","","kg","34"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","780"]
["","","Värme","Superlåg","varv/min","740"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Värme","Omgivning","Min.","°CVT","-15"]
["","","","Max.","°CVT","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","46"]
["","Värme","","Hög","dBA","47"]
["","","","Låg","dBA","44"]
["Köldmedium","Typ","","","","R-410A"]
["","Mängd","","","kg","1.0"]
["","Mängd","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","15"]
["Standardtillbehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]