{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Ineffekt","Kyla","","Nom.","kW","0.019","0.020","0.032"]
["","Värme","","Nom.","kW","0.023","0.023","0.032"]
["Hölje","Färg","","","","Vit","Vit","Vit"]
["Mått","Enhets-","","Höjd","mm","286","286","286"]
["","","","Bredd","mm","770","770","770"]
["","","","Djup","mm","225","225","225"]
["Vikt","Enhet","","","kg","8.50","8.50","9.00"]
["Fläkt","Luftflöde","Kyla","Hög","m³/min","9.5","9.7","11.5"]
["","","","Medel","m³/min","7.4","7.7","8.3"]
["","","","Låg","m³/min","5.6","5.8","6.3"]
["","","","Tyst drift","m³/min","4.2","4.2","4.5"]
["","","Värme","Hög","m³/min","10.4","10.4","11.5"]
["","","","Medel","m³/min","8.1","8.1","9.0"]
["","","","Låg","m³/min","6.2","6.4","7.0"]
["","","","Tyst drift","m³/min","5.2","5.2","5.1"]
["Ljudeffektsnivå","Kyla","","","dBA","55","55","58"]
["","Värme","","","dBA","55","55","58"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","39","40","43"]
["","","","Medel","dBA","33","33","34"]
["","","","Låg","dBA","25","26","27"]
["","","","Tyst drift","dBA","19","19","20"]
["","Värme","","Hög","dBA","39","40","40"]
["","","","Medel","dBA","34","34","35"]
["","","","Låg","dBA","28","28","29"]
["","","","Tyst drift","dBA","21","21","21"]
["Röranslutningar","Vätska","","YD","mm","6","6","6"]
["","Gas","","YD","mm","9.50","9.50","9.50"]
["","Kondensvatten","","","","18","18","18"]
["Styrsystem","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardtillbehör","Installationsanvisning","","","","1","1","1"]
["","Bruksanvisning","","","","1","1","1"]
["","Infraröd fjärrkontroll","","","","1","1","1"]
["","AAA torrbatterier","","","","2","2","2"]
["","Hållare för fjärrkontroll","","","","1","1","1"]
["","Monteringsplåt","","","","1","1","1"]
["","Luftreningsfilter med titanapatit","","","","1","1","1"]
["","Silverpartikelfilter","","","","1","1","1"]
["","Fästskruvar för inomhusenhet","","","","2","2","2"]
["","Allmänna säkerhetsföreskrifter","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemperatur 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m (horisontellt)","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m (horisontellt)","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m (horisontellt)"]
["","","","","","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data"]