{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","AVA125AMVE / AZAS125M7V1B"]
["Kylkapacitet","Nom.","","kW","12.1 (1)"]
["Värmekapacitet","Nom.","","kW","13.5 (2)"]
["Rumskyla","Kapacitet","Pdesign","kW","12.1"]
["","SEER","","","5.30"]
["","Årlig energiförbrukning","","kWh/a","1,370"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.00"]
["","SCOP/A","","","3.64"]
["","Årlig energiförbrukning","","kWh/a","2,308"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data"]