{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["Mått","Enhet","","Höjd","mm","990","990","990"]
["","","","Bredd","mm","940","940","940"]
["","","","Djup","mm","320","320","320"]
["Vikt","Enhet","","","kg","","70"]
["Compressor","Typ","","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-5","-5","-5"]
["","","","Max.","°CTT","46","46","46"]
["","Värme","Omgivning","Min.","°CVT","-15","-15","-15"]
["","","","Max.","°CVT","15.5","15.5","15.5"]
["Ljudeffektsnivå","Kyla","","","dBA","70","71","73"]
["","Värme","","","dBA","","71","73 (1)"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","53","53","54"]
["","Värme","","Nom.","dBA","57","57","57"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","Mängd","","","kg","2.60","2.60","2.90"]
["Köldmedium","GWP","","","","","675"]
["Köldmedium","Mängd","","","tCO2Eq","1.76","1.76","1.96"]
["Röranslutningar","Vätska","","YD","mm","9.52","9.52","9.52"]
["Röranslutningar","Gas","","YD","mm","","15.9"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","30","30","30"]
["","","System","Motsvarande","m","50","50","50"]
["","","","Ingen extra laddning","m","30","30","30"]
["","Extra köldmediemängd","","","kg/m","Se installationsmanual","Se installationsmanual","Se installationsmanual"]
["","Nivåskillnad","IU - OU","Max.","m","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5"]
["Standardtillbehör","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Strömförsörjning","Fas","","","","3~","3~","3~"]
["","Strömförsörjning-=-Frequency","","Frequency","","50","50","50"]
["","Strömförsörjning-=-Spänning","","Spänning","","380-415","380-415","380-415"]
["Ström - 50Hz","Ström - 50Hz-=-Maximal säkringsström (MFA)","","Ström - 50Hz-=-Maximal säkringsström (MFA)-=-A","","","16"]
["Anm:","","","","","","(1) - Enligt ENER Lot 21","(1) - Enligt ENER Lot 21"]
["Vikt","Enhet","","","kg","70","","77"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor"]
["Köldmedium","GWP","","","","675","","675"]
["Röranslutningar","Gas","","YD","mm","15.9","","15.9"]
["Ström - 50 Hz","Max amperestyrka i säkring (MFA)","","","A","16","","16"]