{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000554"]
[]
[]
[]
[]
["","","","","","BR00000554."]
["Tillämpning","","","","","Golvmonterad typ"]
["Effekt","m³/min","","","","33.33"]
["Hölje","Färg","","","","Målad galvaniserad stålplåt"]
["Mått","Enhet","","Höjd","mm","1628"]
["","","","Bredd","mm","720"]
["","","","Djup","mm","770"]
["Vikt","Enhet","","","kg","150"]
["Tillämplig rumsstorlek","m²","","","","133"]
["Luftrening","Ineffekt","","H","kW","0.379"]
["Ljudtrycksnivå","Luftrening","","Hög","dBA","55.9"]
["Fläkt","Luftflödeshastighet","Luftrening","Turbo","m³/h","2300"]
["","","","Hög","m³/h","2000"]
["Dammuppsamlingsmetod","","","","","Förfilter RedPleat, ISO Coarse 70% 592x592x45, H14 HEPA-filtrering"]
["Säkerhetskomponenter","Punkt","","01","","Säkerhetsbrytare (driften stoppar när bakre dörr öppnas)"]
["Standardtillbehör","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Nätsladd","m","","","","3"]
["Strömförsörjning","Frequency","","","Hz","50/60"]
["Belastningsström","Luftrening","","Hög","A","1.73"]