{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":7,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 5MXM-N9"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 5MXM90N2V1B9","CHYHBH08AFV32 / 5MXM90N2V1B9"]
["Tappvattenvärmning","Allmänt","","Deklarerad belastningsprofil","","XL","XL"]
["","Medelklimat","","Energieffektivitetsklass för vattenuppvärmning","","A","A"]
["COP","","","","","4.04 (1)","4.17 (1)"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","Seasonal space heating eff. class","","A+","A+"]
["","","","ηs (årstidsrelaterad verkningsgrad)","%","120.8","120.8"]
["","","","SCOP","","3.09","3.09"]
["Värmekapacitet","Nom.","","","kW","4.50 (1)","6.78 (1)"]
["Anm:","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), värmare förbikopplad","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), värmare förbikopplad"]