{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Ljudtrycksnivå","Värme","Hög","dBA","39"]
["","","Medel","dBA","32"]
["","","Tyst drift","dBA","21"]
["","","Låg","dBA","25"]
["","Kyla","Medium","dBA","32"]
["","","Tyst drift","dBA","21"]
["","","Låg","dBA","25"]
["","","Hög","dBA","39"]
["Standardtillbehör","Installationsanvisning","","","1"]
["","Bruksanvisning","","","1"]
["","Luftfilter","","","2"]
["","Infraröd fjärrkontroll","","","1"]
["","Fjärrkontrollens monteringsplåt","","","1"]
["","Skruvpåse","","","1"]
["","Skruvlock","","","1"]
["","AAA torrbatterier","","","2"]
["","Allmänna säkerhetsföreskrifter","","","1"]
["Köldmedium","GWP","","","675.0"]
["Styrsystem","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Röranslutningar","Vätska","YD","mm","6.35"]
["","Gas","YD","mm","9.50"]
["","Kondensvatten","","","18"]
["Ineffekt","Kyla","Nom.","kW","0.020"]
["","Värme","Nom.","kW","0.020"]
["Ljudeffektsnivå","Kyla","","dBA","57"]
["Mått","Enhet","Bredd","mm","798"]
["","","Djup","mm","189"]
["","","Höjd","mm","295"]
["Hölje","Colour","","","Svart trä"]
["Vikt","Enhet","","kg","12"]
["Power supply","Phase","","","1~"]
["","Frequency","","Hz","50"]
["","Namn","","","V1"]
["","Spänning","","V","220-240"]