{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 3MXM-A9"]
[]
[]
[]
[]
["","","","","CTXM15R2V1B / CTXM15R2V1B / CTXM15R2V1B / 3MXM40A2V1B9","CTXM15R5V1B / CTXM15R5V1B / CTXM15R5V1B / 3MXM40A2V1B9"]
["Kylkapacitet","Nom.","","kW","4.00","4.00"]
["Värmekapacitet","Nom.","","kW","4.60","4.60"]
["Nominell verkningsgrad","EER köldfaktor","","","5.18","5.18"]
["","COP","","","5.17","5.17"]
["","Årlig energiförbrukning","","kWh","386","386"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Rumskyla","Energieffektivitetsklass","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","4.00","4.00"]
["","SEER","","","8.55","8.55"]
["","Årlig energiförbrukning","","kWh/a","164","164"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A++","A++"]
["","Kapacitet","Pdesign","kW","4.90","4.90"]
["","SCOP/A","","","4.65","4.65"]
["","Pdh Värmekapacitet vid -10°","","kW","4.00","4.00"]
["","Årlig energiförbrukning","","kWh/a","1475","1475"]
["Intervall för energieffektivitet","","","","A+++ ~ D","A+++ ~ D"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]