{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Omgivningstemperatur","Relativ luftfuktighet <","","","%","85"]
["Max. antal inomhusdelar","","","","","32"]
["Effektförbrukning","kW","","","","0.015 (1)"]
["Kommunikation","DIII-NET","","Kvantitet","","1"]
["","","","Uppmärksamma","","DIII-NET (F1F2)"]
["","Ethernet","","Kvantitet","","1"]
["","Ingångsterminal","Digital","Kvantitet","","4"]
["Mått","Enhet","","Bredd","mm","384"]
["","","","Djup","mm","92"]
["","","","Höjd","mm","136"]
["Max. antal anslutningsbara utomhusenheter","","","","","7"]
["Power supply","Frequency","","","Hz","50/60"]
["","Spänning","","","V","110-240 AC"]
["Anm:","","","","","(1) - Ingår ingång för strömförsörjning från WAGO kraftaggregat, CPU-modul samt I/O-modul"]
["","","","","","(2) - Måtten innefattar WAGO kraftaggregat, CPU-modul, I/O-modul samt nödvändigt utrymme mellan det olika delarna"]
["","","","","","(3) - Måtten på skärmen tom tillval är: höjd: 209 mm, bredd: 123 mm, djup: 8,5 mm"]