{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Ingång","Typ","","","","Touchpanel (10 bitars avkodad analog ingång)"]
["Omgivningstemperatur","Relativ luftfuktighet <","","","%","85"]
["","Drift","","Min.","°C","0"]
["","","","Max.","°C","40"]
["Max. antal inomhusdelar","","","","","64, 128 (1)"]
["Kommunikation","DIII-NET","","Kvantitet","","1"]
["","","","Uppmärksamma","","Kommunikationslinje för luftkonditioneringsutrustning"]
["","10BASE-T","","Uppmärksamma","","Webbalternativ"]
["","Ethernet","","Uppmärksamma","","Port för Webben och e-post"]
["","Ingångsterminal","Digital","Kvantitet","","1"]
["","","","Uppmärksamma","","Tvingad nedstängning"]
["","","Puls","Kvantitet","","3"]
["","","","Uppmärksamma","","Effektmätande puls"]
["","Modem","","Uppmärksamma","","Inbyggd modemfunktion"]
["","PCMCIA","","Uppmärksamma","","Flashminneskort"]
["","RS-232C","","Uppmärksamma","","DIII-NET PLUS adapter"]
["Mått","Enhet","","Bredd","mm","230"]
["","","","Djup","mm","107"]
["","","","Höjd","mm","147"]
["LCD","Typ","","","","QVGA (320 x 240), 4 096 färger"]
["","Dimensioner","","Bredd","Återflöde","5.7"]
["Max. antal anslutningsbara utomhusenheter","","","","","10, 20 (1)"]
["Power supply","Frequency","","","Hz","50/60"]
["","Spänning","","","V","100-240 (tillhandahålls externt)"]
["Anm:","","","","","(1) - Kombinerat med DCS601A51"]