{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA04-08EV3"]
[]
[]
[]
[]
["","","","","","EDLA04E2V3","EDLA06E2V3","EDLA08E2V3"]
["Värmekapacitet","Nom.","","","kW","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)"]
["Ineffekt","Värme","","Nom.","kW","0.840 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Mått","Enhet","","Höjd","mm","770","770","770"]
["","","","Bredd","mm","1250","1250","1250"]
["","","","Djup","mm","362","362","362"]
["Vikt","Enhet","","","kg","88","88","88"]
["Driftsområde","Värme","Vattensida","Min.","°C","9 (3)","9 (3)","9 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)"]
["","Tappvarmvatten","Omgivning","Min.","°CTT","-27","-27","-27"]
["","","","Max.","°CTT","35","35","35"]
["","","Vattensida","Min.","°C","25","25","25"]
["","","","Max.","°C","55 (3)","55 (3)","55 (3)"]
["Ljudeffektsnivå","Värme","","Nom.","dBA","58.0 (1)","60.0 (1)","62.0 (1)"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","44.0 (1)","47.0 (1)","49.0 (1)"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Mängd","","","kg","1.35","1.35","1.35"]
["","Mängd","","","tCO2Eq","0.91","0.91","0.91"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.26","3.26","3.32"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A++","A++","A++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","4.48","4.47","4.56"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++","A+++"]
["Kompressorkomponent","Huvudströmförsörjning","","Fas","","3N","3N","3N"]
["","","","Spänning","V","220","220","220"]
["Strömförsörjning","Namn","","","","V3","V3","V3"]
["","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","230 +/-10%","230 +/-10%","230 +/-10%"]
["Anm:","","","","","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(3) - För mer information se driftsområdesritning","(3) - För mer information se driftsområdesritning","(3) - För mer information se driftsområdesritning"]