{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAH-D9W"]
[]
[]
[]
[]
["","","","","","EGSAH06DA9W","EGSAH10DA9W"]
["Värmekapacitet","Min.","","","kW","0.85","0.85"]
["","Nom.","","","kW","3.35","5.49"]
["","Max.","","","kW","7.98","9.55"]
["Ineffekt","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.7"]
["Hölje","Färg","","","","Vit +  svart","Vit +  svart"]
["","Material","","","","Förbehandlad plåt"]
["Mått","Enhet","","Höjd","mm","1891","1891"]
["","","","Bredd","mm","597","597"]
["","","","Djup","mm","666","666"]
["Vikt","Enhet","","","kg","222","222"]
["Tank","Vattenvolym","","","l","180","180"]
["","Isolering","","Värmeförlust","kWh/24 h","1.2","1.2"]
["","Korrosionsskydd","","","","Betning","Betning"]
["Köldmedium","Typ","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Mängd","","","tCO2Eq","1.15","1.15"]
["","Mängd","","","kg","1.70","1.70"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.72 (1)","4.00 (1)"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A++","A+++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","5.06 (1)","5.12 (1)"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++"]
["Strömförsörjning","Fas","","","","1~/3~","1~/3~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","230/400","230/400"]
["Aktuell","Rekommenderade säkringar","","","A","16/32","16/32"]
["Anm:","","","","","(1) - I enlighet med EN14825 och EN14511:=2018","(1) - I enlighet med EN14825 och EN14511:=2018"]