{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9WG"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9WG","EGSAX10DA9WG"]
["Värmekapacitet","Min.","","","kW","0.85"]
["","Nom.","","","kW","3.35"]
["","Max.","","","kW","7.98"]
["Ineffekt","Nom.","","","kW","0.74"]
["COP","","","","","4.51"]
["Hölje","Färg","","","","Grey + Black"]
["Mått","Enhet","","Höjd","mm","1,891"]
["","","","Bredd","mm","597"]
["","","","Djup","mm","666"]
["Vikt","Enhet","","","kg","222"]
["Tank","Vattenvolym","","","l","180"]
["","Isolering","","Värmeförlust","kWh/24 h","1.2"]
["","Korrosionsskydd","","","","Betning"]
["Köldmedium","Typ","","","","R-32"]
["","GWP","","","","675.0"]
["","Mängd","","","kg","1.70"]
["Driftsområde","Installationsutrymme","","Min.","°C","5"]
["","","","Max.","°C","35"]
["","Köldbärarsida","","Min.","°C","-10"]
["","","","Max.","°C","30"]
["","Värme","Vattensida","Min.","°C","5"]
["","","","Max.","°C","65"]
["","Tappvarmvatten","Vattensida","Min.","°C","25"]
["","","","Max.","°C","60"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.77 (1)"]
["","","","Seasonal space heating eff. class","","A++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","5.18 (1)"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++"]
["Power supply","Fas","","","","1~/3~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","230/400"]
["Ström","Rekommenderade säkringar","","","A","16/32"]
["Anm:","","","","","(1) - I enlighet med EN14825 och EN14511:=2018"]
["","","","","","(2) - Se driftområdesritning: området ökar med hjälp av en booster-värmare eller en backupvärmare"]
["Värmekapacitet","Min.","","","kW","","0.85"]
["","Nom.","","","kW","","5.49"]
["","Max.","","","kW","","9.55"]
["Ineffekt","Nom.","","","kW","","1.17"]
["COP","","","","","","4.7"]
["Hölje","Färg","","","","","Grå + svart"]
["Mått","Enhet","","Höjd","mm","","1891"]
["","","","Bredd","mm","","597"]
["","","","Djup","mm","","666"]
["Vikt","Enhet","","","kg","","222"]
["Tank","Isolering","","Värmeförlust","kWh/24 h","","1.2"]
["","Korrosionsskydd","","","","","Betning"]
["Köldmedium","Typ","","","","","R-32"]
["","GWP","","","","","675.0"]
["","Mängd","","","tCO2Eq","","1.15"]
["","Mängd","","","kg","","1.70"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","","4.05 (1)"]
["","","","Klass för årstidsrelaterad verkningsgrad","","","A+++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","","5.20 (1)"]
["","","","Klass för årstidsrelaterad verkningsgrad","","","A+++"]
["Strömförsörjning","Fas","","","","","1~/3~"]
["","Frequency","","","Hz","","50"]
["","Spänning","","","V","","230/400"]
["Aktuell","Rekommenderade säkringar","","","A","","16/32"]
["Anm:","","","","","","(1) - I enlighet med EN14825 och EN14511:=2018"]