{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Ljudtrycksnivå","Nom.","","","dBA","32.0 (6)"]
["Köldmedium","GWP","","","","2,090"]
["","Mängd","","","kg","1.80"]
["","Typ","","","","R-410A"]
["Driftsområde","Installationsutrymme","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Värme","Vattensida","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Köldbärarsida","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Tappvarmvatten","Vattensida","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Ineffekt","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Sound power level","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Mått","Enhet","","Bredd","mm","600"]
["","","","Djup","mm","728"]
["","","","Höjd","mm","1,730"]
["Hölje","Material","","","","Förbehandlad plåt"]
["","Färg","","","","Vit"]
["Tank","Vattenvolym","","","l","180"]
["","Korrosionsskydd","","","","Anod"]
["","Isolering","","Värmeförlust","kWh/24 h","1.36 (4)"]
["Vikt","Enhet","","","kg","210"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 35°C","Allmänt","ηs (årstidsrelaterad verkningsgrad)","%","194"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++"]
["","","","SCOP","","5.06"]
["","Framledningstemperatur vid medelklimat 55°C","Allmänt","Seasonal space heating eff. class","","A++"]
["","","","ηs (årstidsrelaterad verkningsgrad)","%","139"]
["","","","SCOP","","3.68"]
["Värmekapacitet","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Fas","","","","3~"]
["","Namn","","","","9W"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","400"]
["Ström","Rekommenderade säkringar","","","A","25"]
["Anm:","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - med 40% propylenglykol"]
["","","","","","(4) - Värmeförlust enligt EN12897"]
["","","","","","(5) - Inklusive rörledning + PHE + backupvärmare/exklusive expansionskärl"]
["","","","","","(6) - Ljudtrycksnivån mäts med en mikrofon på 1 m avstånd från enheten. Det är ett relativt värde som beror på avståndet och omgivningens akustik."]
["","","","","","(7) - Från värmepump"]
["","","","","","(8) - Från värmepump + backupvärmare"]
["","","","","","(9) - Från backupvärmare"]