{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-E"]
[]
[]
[]
[]
["","","","","","EHSHB04P30EG","EHSHB08P30EG","EHSHB08P50EG","EHSHB04P30EF (Archived)","EHSHB08P30EF (Archived)","EHSHB08P50EF (Archived)"]
["Hölje","Färg","","","","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)"]
["","Material","","","","Stryktålig polypropylen","Stryktålig polypropylen","Stryktålig polypropylen","Stryktålig polypropylen","Stryktålig polypropylen","Stryktålig polypropylen"]
["Mått","Enhet","","Höjd","mm","1891","1891","1910","1892","1892","1905"]
["","","","Bredd","mm","594","594","792","594","594","792"]
["","","","Djup","mm","644","644","817","644","644","812"]
["Vikt","Enhet","","","kg","80.0","80.0","104","79","79","110"]
["PED","Kategori","","","","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["","Mängd","","","kg","1.50","1.50","1.50","1.5","1.5","1.5"]
["Ljudeffektsnivå","Nom.","","","dBA","39","39","39","39","39","39"]
["Driftsområde","Värme","Vattensida","Min.","°C","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65"]
["","Kyla","Omgivning","Min.","°CTT","10","10","10","10","10","10"]
["","","Vattensida","Min.","°C","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Spänning","","","V","230","230","230","230","230","230"]
["Anm:","","","","","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897"]