{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHSX08P30EF / ERGA06EAV3H","EHSX08P50EF / ERGA06EAV3H","EHSX08P30EG / ERGA06EAV3H","EHSX08P50EG / ERGA06EAV3H"]
["Inomhusdel","","","","","EHSX08P30EF","EHSX08P50EF","EHSX08P30EG","EHSX08P50EG"]
["Värmekapacitet","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Kylkapacitet","Nom.","","","kW","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)"]
["Ineffekt","Värme","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["","Kyla","","Nom.","kW","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["EER","","","","","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)"]
["Tappvattenvärmning","Allmänt","","Deklarerad belastningsprofil","","L","XL","L","XL"]
["","Medelklimat","","Energieffektivitetsklass för vattenuppvärmning","","A+","A+","A+","A+"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.28","3.28","3.28","3.28"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A++","A++","A++","A++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","4.52","4.52","4.52","4.52"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++","A+++","A+++"]
["Anm:","","","","","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]