{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA6VG / ERGA04EAV3A","EHVX04S23EA6VG / ERGA04EAV3A","EHVX08S18EA6VG / ERGA06EAV3A","EHVX08S23EA6VG / ERGA06EAV3A","EHVX08S18EA6VG / ERGA08EAV3A","EHVX08S23EA6VG / ERGA08EAV3A"]
["Värmekapacitet","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Kylkapacitet","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)"]
["Ineffekt","Värme","","Nom.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Kyla","","Nom.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)"]
["Effektförbrukning","Varmvatten från 10°C till 50°C","","Nom.","kWh","2.48","3.01","2.48","3.01","2.48","3.01"]
["Uppvärmning från 10°C till 50°C","hr","","","","1h28min","1h40min","1h28min","1h40min","1h28min","1h40min"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.40 (1), 3.14 (2)","5.40 (1), 3.14 (2)"]
["Tappvattenvärmning","Allmänt","","Deklarerad belastningsprofil","","L","XL","L","XL","L","XL"]
["","Medelklimat","","Energieffektivitetsklass för vattenuppvärmning","","A+","A+","A+","A+","A+","A+"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.29","3.29","3.27","3.27","3.3","3.3"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A++","A++","A++","A++","A++","A++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","4.54","4.54","4.52","4.52","4.61","4.61"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Intervall för energieffektivitet","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Anm:","","","","","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]