{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV3"]
[]
[]
[]
[]
["","","","","","EKHH2E260AAV3"]
["Sound power level","Tappvattenvärmning","","Inomhusenhet","dBA","53"]
["","","","Utomhusenhet","dBA","52"]
["Tappvattenvärmning","Allmänt","","Energieffektivitetsklass vattenvärmning","","A+"]
["","","","Termostattemperaturinställning","°C","55"]
["","","","Deklarerad belastningsprofil","","XL"]
["","Kallt klimat","","AEC (Årlig elförbrukning)","kWh","1,826"]
["","Varmt klimat","","AEC (Årlig elförbrukning)","kWh","1,296"]
["","Medelklimat","","AEC (Årlig elförbrukning)","kWh","1,323"]
["Ekvivalent varmvatten","Max","","","l","342"]
["Värmepump","Automatic defrost start","","","°C","-2"]
["","Driftsområde","Omgivning","Min.","°CTT","-7"]
["","","","Max.","°CTT","38"]
["","Casing","","Material","","Lock: EPP ytbehandling"]
["","","","Färg","","White body / black top"]
["","Systemtryck","","Max.","stång","7"]
["","Avfrostningsmetod","","","","Aktiv med hetgasventil"]
["COP","","","","","3.10 (1), 3.60 (2)"]
["Köldmedium","GWP","","","","1,430.0"]
["","Mängd","","","kg","0.900"]
["","Typ","","","","R-134a"]
["Kompressor","Typ","","","","Rotary non-inverter"]
["Mått","Enhet","","Diameter","mm","650"]
["","","","Höjd","mm","2,000"]
["Varmvatten för hushållet","Uteffekt","","Nom","kW","1.8"]
["Tank","Installation","","Solvärmeanslutning möjlig","","Nej"]
["","Integrerad värmeelementseffekt","","Nom.","kW","1.5"]
["","Hölje","","Material","","Mönstrad ABS"]
["","","","Färg","","Vit"]
["","Dimensioner","Enhet","Höjd","mm","1,500"]
["","Driftsområde","Vattensida","Max.","°C","56"]
["","","","Min.","°C","10"]
["Vikt","Paketerad enhet","","","kg","115"]
["","Enhets-","","Tom","kg","95"]
["","","","Full","kg","349"]
["Installationsplats","","","","","Inomhus"]
["IP class","","","","","IP-X4"]
["Allmänt","Produktbeskrivning","","Luft-till-vatten värmepump","","Ja"]
["","Leverantör/tillverkare","","Namn och adress","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Uppvärmningstid","Max.","","","hh:mm","10:14:00, 07:56:46"]
["Värmepump","Strömförsörjning","","Frekvens","Hz","50"]
["","","","Maximal belastningsström","A","2"]
["","","","Fas","","1P"]
["","","","Spänning","V","230"]
["Tank","Strömförsörjning","","Fas","","1P"]
["","","","Frekvens","Hz","50"]
["","","","Spänning","V","230"]
["Anm:","","","","","(1) - Enligt EN16147-2011, inloppstemperatur 7 °C, rumstemperatur 20 °C, kallvatteninlopp 10 °C"]
["","","","","","(2) - Enligt EN16147-2011, inloppstemperatur 15°C, rumstemperatur 20 °C, kallvatteninlopp 10 °C"]
["","","","","","(3) - Inomhustemperatur: 29°CTT, 19°CVT; utomhustemperatur : 46°CTT, 24°CVT"]
["","","","","","(4) - Inomhustemperatur: 27°CTT, 19°CVT; utomhustemperatur : 35°CTT, 24°CVT"]