{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWCB-B"]
[]
[]
[]
[]
["","","","","","EKHWCB500BA"]
["Montering","","","","","Golv"]
["Hölje","Colour","","","","Trafikvit (RAL9016)/mörkgrå (RAL7011)"]
["","Material","","","","Stryktålig polypropylen"]
["Mått","Enhets-","Höjd","Tank","mm","1,660"]
["","","","Bredd","mm","790"]
["","","","Djup","mm","790"]
["Vikt","Enhets-","","Tom","kg","80"]
["","","","Full","kg","580"]
["Tank","Vattenvolym","","","l","477"]
["","Material","","","","Polypropylen"]
["","Maximal vattentemperatur","","","°C","85"]
["","Klass för energieffektivitet","","","","B"]
["Värmeväxlare","Tappvarmvatten","","Kvantitet","","1"]
["","","","Rörmaterial","","Rostfritt stål (DIN 1.4404)"]
["","","","Intern volym i spole","l","25.8"]
["","","","Driftstryck","stång","6"]
["","","","Medelvärde på specifik termisk uteffekt","W/K","2,580"]
["","Påfyllning","","Kvantitet","","1"]
["","","","Rörmaterial","","Rostfritt stål (DIN 1.4404)"]
["","","","Intern volym i spole","l","9"]
["","","","Driftstryck","stång","3"]
["","","","Medelvärde på specifik termisk uteffekt","W/K","1,030"]
["","Extra solvärme","","Kvantitet","","1"]
["","","","Rörmaterial","","Rostfritt stål (DIN 1.4404)"]
["","","","Intern volym i spole","l","4"]
["","","","Driftstryck","stång","3"]
["","","","Medelvärde på specifik termisk uteffekt","W/K","350"]
["Anm:","","","","","(1) - Värmeförlust enligt EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - För avtappningsvolym 140 l -> 5820 Wh (bad) / 8 kW värmepump"]
["","","","","","(6) - För avtappningsvolym 90 l -> 3660 Wh (bad) / 8 kW värmepump"]
["","","","","","(7) - För avtappningsvolym 140 l -> 5820 Wh (bad) / 16 kW värmepump"]
["","","","","","(8) - För avtappningsvolym 90 l -> 3660 Wh (bad) / 16 kW värmepump"]