{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWMX-C"]
[]
[]
[]
[]
["","","","","EKHWMX300CA","EKHWMX500CA"]
["Ljudtrycksnivå","Nom.","","dBA","28 (5), 28 (6)","28 (5), 32 (6)"]
["Sound power level","Nom.","","dBA","42 (5), 42 (6)","42 (5), 46 (6)"]
["Mått","Enhet","Bredd","mm","595","790"]
["","","Djup","mm","615","790"]
["","","Höjd","mm","1,891","1,896"]
["Hölje","Material","","","Stryktålig polypropylen","Stryktålig polypropylen"]
["","Colour","","","Trafikvit (RAL9016)/mörkgrå (RAL7011)","Trafikvit (RAL9016)/mörkgrå (RAL7011)"]
["Vikt","Enhet","","kg","66","85"]
["Power supply","Fas","","","1~","1~"]
["","Frequency","","Hz","50","50"]
["","Namn","","","V3","V3"]
["","Spänning","","V","230","230"]
["Anm:","","","","(1) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(1) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","(4) - Uppvärmning av tank med endast värmepump, ingen elpatron","(4) - Uppvärmning av tank med endast värmepump, ingen elpatron"]
["","","","","(5) - EBLQ05C2V3","(5) - EBLQ05C2V3"]
["","","","","(6) - EBLQ07C2V3","(6) - EBLQ07C2V3"]