{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPSK06ARV3","EPSK08ARV3","EPSK10ARV3"]
["Mått","Enhet","","Höjd","mm","1123","1123","1123"]
["","","","Bredd","mm","1330","1330","1330"]
["","","","Djup","mm","604","604","604"]
["Vikt","Enhet","","","kg","174","174","174"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","75.7","75.7","75.7"]
["","","Kyla","Hög","m³/min","75.7","75.7","75.7"]
["Driftsområde","Kyla","","Min.","°CTT","10","10","10"]
["","","","Max.","°CTT","43","43","43"]
["","Tappvarmvatten","","Min.","°CTT","-28","-28","-28"]
["","Varmvatten för hushållet","","Max.","°CTT","40","40","40"]
["Ljudeffektsnivå","Värme","","Nom.","dBA","45 (1)","45 (1)","47 (1)"]
["","Kyla","","Nom.","dBA","52.2 (2)","53 (2)","53.2 (2)"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","32.6 (1)","32.4 (1)","32.8 (1)"]
["","Kyla","","Nom.","dBA","36.9 (2)","37.2 (2)","37.3 (2)"]
["Köldmedium","Typ","","","","R-290","R-290","R-290"]
["","GWP","","","","3","3","3"]
["","Mängd","","","tCO2Eq","0.003","0.003","0.003"]
["","Mängd","","","kg","1","1","1"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","10","10","10"]
["Strömförsörjning","Namn","","","","V3","V3","V3"]
["","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","230","230","230"]
["Aktuell","Rekommenderade säkringar","","","A","25","25","25"]
["Anm:","","","","","(1) - Uppmätt vid LWC 47-55°C; Ta DB/WB 7°C/6°C","(1) - Uppmätt vid LWC 47-55°C; Ta DB/WB 7°C/6°C","(1) - Uppmätt vid LWC 47-55°C; Ta DB/WB 7°C/6°C"]
["","","","","","(2) - Uppmätt vid LWC 12-7°C; Det är 35°C.","(2) - Uppmätt vid LWC 12-7°C; Det är 35°C.","(2) - Uppmätt vid LWC 12-7°C; Det är 35°C."]
["","","","","","(3) - 1 1/4\" fältanslutning","(3) - 1 1/4\" fältanslutning","(3) - 1 1/4\" fältanslutning"]
["","","","","","(4) - 1 1/2\" fältanslutning","(4) - 1 1/2\" fältanslutning","(4) - 1 1/2\" fältanslutning"]