{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3A","ERGA06EAV3A","ERGA08EAV3A"]
["Mått","Enhet","","Höjd","mm","740","740","740"]
["","","","Bredd","mm","884","884","884"]
["","","","Djup","mm","388","388","388"]
["Vikt","Enhet","","","kg","58.5","58.5","58.5"]
["Driftsområde","Kyla","","Min.","°CTT","10","10","10"]
["","","","Max.","°CTT","43","43","43"]
["","Tappvarmvatten","","Min.","°CTT","-25","-25","-25"]
["","Varmvatten för hushållet","","Max.","°CTT","35","35","35"]
["Ljudeffektsnivå","Värme","","Nom.","dBA","58 (1)","60 (1)","62 (1)"]
["","Kyla","","Nom.","dBA","61 (1)","62 (1)","62 (1)"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","44 (1)","47 (1)","49 (1)"]
["","Kyla","","Nom.","dBA","48 (1)","49 (1)","50 (1)"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Mängd","","","tCO2Eq","1.01","1.01","1.01"]
["","Mängd","","","kg","1.5","1.5","1.5"]
["Röranslutningar","Vätska","","YD","mm","6","6","6"]
["","Gas","","YD","mm","15.9","15.9","15.9"]
["","Kondensvatten","","YD","mm","18","18","18"]
["","Nivåskillnad","IU - OU","Max.","m","20.0","20.0","20.0"]
["","Värmeisolering","","","","Rör för både vätska och gas","Rör för både vätska och gas","Rör för både vätska och gas"]
["Strömförsörjning","Namn","","","","V3","V3","V3"]
["","Fas","","","","1N~","1N~","1N~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","230","230","230"]
["Aktuell","Rekommenderade säkringar","","","A","16","16","16"]
["Anm:","","","","","(1) - Kyla Ta 35 °C - LWE 18°C ( DT = 5 °C ); Värme Ta DB/WB 7 °C/6 °C - LWC 35°C ( DT = 5 °C)","(1) - Kyla Ta 35 °C - LWE 18°C ( DT = 5 °C ); Värme Ta DB/WB 7 °C/6 °C - LWC 35°C ( DT = 5 °C)","(1) - Kyla Ta 35 °C - LWE 18°C ( DT = 5 °C ); Värme Ta DB/WB 7 °C/6 °C - LWC 35°C ( DT = 5 °C)"]