{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E"]
[]
[]
[]
[]
["","","","","","ETSXB16P50EF","ETSXB16P30EF"]
["Hölje","Colour","","","","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)"]
["","Material","","","","Stryktålig polypropylen","Stryktålig polypropylen"]
["Mått","Enhets-","","Höjd","mm","1,910","1,892"]
["","","","Bredd","mm","792","594"]
["","","","Djup","mm","816","644"]
["Vikt","Enhet","","","kg","100","76"]
["Ljudeffektsnivå","Nom.","","","dBA","45.6","45.6"]
["Ljudtrycksnivå","Nom.","","","dBA","32.8","32.8"]
["Driftsområde","Heating","Vattensida","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["","Kyla","Omgivning","Min.","°CTT","0 (2)","0 (2)"]
["","","Vattensida","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["Power supply","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","230","230"]
["Anm:","","","","","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897"]
["","","","","","(2) - Se ritningar över driftsbegränsning","(2) - Se ritningar över driftsbegränsning"]