{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":9,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYA-DW1P-H-"]
[]
[]
[]
[]
["","","","","","EWYA009DAW1P-H-","EWYA011DAW1P-H-","EWYA014DAW1P-H-","EWYA016DAW1P-H-"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","44.0","47.7","50.8","51.0"]
["Hydrauliska komponenter","Expansionskärl","","Volym","l","8","8","8","8"]
["Driftsområde","Omgivande luft","Kyla","Min.","°CTT","10","10","10","10"]
["","","","Max.","°CTT","43","43","43","43"]
["","","Värme","Max.","°CTT","25","25","25","25"]
["","","","Min.","°CTT","-25","-25","-25","-25"]
["","Vattensida","Värme","Min.","°CTT","9 (7)","9 (7)","9 (7)","9 (7)"]
["","","","Max.","°CTT","60 (7)","60 (7)","60 (7)","60 (7)"]
["","","Kyla","Max.","°CTT","22","22","22","22"]
["","","","Min.","°CTT","5","5","5","5"]
["Köldmediemängd","Per krets","","","kg","3.80","3.80","3.80","3.80"]
["","Refrigerant charge-=-Per circuit-=-TCO2Eq","","","TCO2Eq","2.6","2.6","2.6","2.6"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing inverterkompressor","Hermetiskt tillsluten swing inverterkompressor","Hermetiskt tillsluten swing inverterkompressor","Hermetiskt tillsluten swing inverterkompressor"]
["","Starting method","","","","Inverterdriven","Inverterdriven","Inverterdriven","Inverterdriven"]
["","Kvantitet_","","","","1","1","1","1"]
["Luftvärmeväxlare","Typ","","","","Högeffektiv fläns- och rörtyp med integrerad underkylare","Högeffektiv fläns- och rörtyp med integrerad underkylare","Högeffektiv fläns- och rörtyp med integrerad underkylare","Högeffektiv fläns- och rörtyp med integrerad underkylare"]
["Vikt","Enhet","","","kg","147","147","147","147"]
["EER","","","","","3.35 (1), 5.34 (2)","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Köldmedium","GWP","","","","675.0","675.0","675.0","675.0"]
["","Typ","","","","R-32","R-32","R-32","R-32"]
["","Kretsar","","Kvantitet","","1","1","1","1"]
["","Styrning","","","","Elektronisk expansionsventil","Elektronisk expansionsventil","Elektronisk expansionsventil","Elektronisk expansionsventil"]
["Fläktmotor","Varvtal","Kyla","Nom.","varv/min","500","550","650","650"]
["","","Värme","Nom.","varv/min","400","450","550","650"]
["Nedkylningskapacitet","Nom.","","","kW","9.35 (1), 9.10 (2)","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Vattenvärmeväxlare","Vattenvolym","","","l","2","2","2","2"]
["","Min vattenvolym i systemet","","","l","50 (6)","50 (6)","50 (6)","50 (6)"]
["","Typ","","","","Plattvärmeväxlare","Plattvärmeväxlare","Plattvärmeväxlare","Plattvärmeväxlare"]
["Effektförbrukning","Kyla","","Nom.","kW","2.79 (1), 1.71 (2)","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["","Värme","","Nom.","kW","1.91 (3), 2.43 (4)","2.18 (3), 2.68 (4)","2.46 (3), 3.42 (4)","3.53 (3), 4.56 (4)"]
["Ljudeffektsnivå","Kyla","","Nom.","dBA","65.5","67.0","69.0","69.0"]
["COP","","","","","4.91 (3), 3.71 (4)","4.83 (3), 3.66 (4)","4.87 (3), 3.64 (4)","4.53 (3), 3.51 (4)"]
["Mått","Enhets-","","Bredd","mm","1,380","1,380","1,380","1,380"]
["","","","Djup","mm","460","460","460","460"]
["","","","Höjd","mm","870","870","870","870"]
["Effektstyrning","Metod","","","","Variabel (inverter)","Variabel (inverter)","Variabel (inverter)","Variabel (inverter)"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","","","ηs (årstidsrelaterad verkningsgrad)","%","135","132","134","132"]
["","","","SCOP","","3.44","3.37","3.42","3.37"]
["Fläkt","Luftflödeshastighet","Värme","Nom.","m³/min","48.0","55.8","70.4","85.0"]
["","","Kyla","Nom.","m³/min","63","70","85","85"]
["Värmekapacitet","Nom.","","","kW","9.37 (3), 9.00 (4)","10.6 (3), 9.82 (4)","12.0 (3), 12.5 (4)","16.0 (3), 16.0 (4)"]
["Kompressor","Starting method","","","","Inverter","Inverter","Inverter","Inverter"]
["Power supply","Phase","","","","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Namn","","","","W1","W1","W1","W1"]
["","Spänning","","","V","400","400","400","400"]
["Anm:","","","","","(1) - Kyla: EW 12°C; LW 7°C; omgivningsförhållanden: 35 °CTT","(1) - Kyla: EW 12°C; LW 7°C; omgivningsförhållanden: 35 °CTT","(1) - Kyla: EW 12°C; LW 7°C; omgivningsförhållanden: 35 °CTT","(1) - Kyla: EW 12°C; LW 7°C; omgivningsförhållanden: 35 °CTT"]
["","","","","","(2) - Kyla: EW 23°C; LW 18°C; omgivningsförhållanden: 35 °CTT","(2) - Kyla: EW 23°C; LW 18°C; omgivningsförhållanden: 35 °CTT","(2) - Kyla: EW 23°C; LW 18°C; omgivningsförhållanden: 35 °CTT","(2) - Kyla: EW 23°C; LW 18°C; omgivningsförhållanden: 35 °CTT"]
["","","","","","(3) - Förhållande: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - Förhållande: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - Förhållande: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - Förhållande: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(4) - Förhållande: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Förhållande: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Förhållande: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Förhållande: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(5) - I enlighet med EN14825","(5) - I enlighet med EN14825","(5) - I enlighet med EN14825","(5) - I enlighet med EN14825"]
["","","","","","(6) - Beroende på driftläge, se installationsmanualen.","(6) - Beroende på driftläge, se installationsmanualen.","(6) - Beroende på driftläge, se installationsmanualen.","(6) - Beroende på driftläge, se installationsmanualen."]
["","","","","","(7) - För mer information se driftsområdesritning","(7) - För mer information se driftsområdesritning","(7) - För mer information se driftsområdesritning","(7) - För mer information se driftsområdesritning"]