{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZQSG71L3V1B","FAA100BUV1B / RZQSG100L9V1B"]
["Nedkylningskapacitet","Nom.","","kW","6.80","9.50"]
["Rumskyla","SEER","","","6.05","5.61"]
["","Årlig energiförbrukning","","kWh/a","394","593"]
["","Kapacitet","Pdesign","kW","6.80","9.50"]
["","Energieffektivitetsklass","","","A+","A+"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.33","6.81"]
["","SCOP/A","","","3.90","4.01"]
["","Energieffektivitetsklass","","","A","A+"]
["","Årlig energiförbrukning","","kWh/a","2,123","2,378"]
["Nominell verkningsgrad","EER köldfaktor","","","3.21","3.01"]
["","Årlig energiförbrukning","","kWh","1,059","1,578"]
["","COP","","","3.61","3.41"]
["","Energimärkningsdirektiv","Kyla","","A","B"]
["","","Värme","","A","B"]
["Värmekapacitet","Nom.","","kW","7.50","10.80"]
["Anm:","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m.","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m.","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","(3) - Se separat ritning för driftsområde","(3) - Se separat ritning för driftsområde"]
["","","","","(4) - Se separata ritningar för elektriska data","(4) - Se separata ritningar för elektriska data"]