{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Hölje","Färg","","","","Vit","Vit"]
["","Material","","","","Plast","Plast"]
["Mått","Enhet","","Höjd","mm","290","340"]
["","","","Bredd","mm","1050","1200"]
["","","","Djup","mm","269","262"]
["Vikt","Enhet","","","kg","14","18"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","16.2","23"]
["","","","Medel","m³/min","13.4","21.1"]
["","","","Låg","m³/min","12.1","18.7"]
["","","Värme","Hög","m³/min","16.9","23"]
["","","","Medel","m³/min","14.2","20.9"]
["","","","Låg","m³/min","12.7","18.7"]
["Ljudeffektsnivå","Kyla","","","dBA","61","65"]
["","Värme","","","dBA","61","65"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","45","49"]
["","","","Medel","dBA","42","45"]
["","","","Låg","dBA","40","41"]
["","Värme","","Hög","dBA","45","49"]
["","","","Medel","dBA","42","45"]
["","","","Låg","dBA","40","41"]
["Röranslutningar","Vätska","","YD","mm","9.52","9.52"]
["","Gas","","YD","mm","15.9","15.9"]
["","Kondensvatten","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-240","220-240"]
["Standardtillbehör","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Anm:","","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["Standardtillbehör","Screw cover","","","","","3"]