{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXM50A5V1B","FBA60A2VEB9 / RXM60A5V1B"]
["Kylkapacitet","Nom.","","kW","5.0","5.7"]
["Värmekapacitet","Nom.","","kW","5.5","7"]
["Nominell verkningsgrad","EER köldfaktor","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Årlig energiförbrukning","","kWh","704","819"]
["","Energimärkningsdirektiv","Kyla","","A","A"]
["","","Värme","","A","A"]
["Rumskyla","Energieffektivitetsklass","","","A++","A+"]
["","Kapacitet","Pdesign","kW","5.0","5.7"]
["","SEER","","","6.27","5.91"]
["","Årlig energiförbrukning","","kWh/a","279","336"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A+","A+"]
["","Kapacitet","Pdesign","kW","4.4","4.6"]
["","SCOP/A","","","4.06","4.01"]
["","Pdh Värmekapacitet vid -10°","","kW","3.73","3.99"]
["","Årlig energiförbrukning","","kWh/a","1,517","1607"]
["Anm:","","","","","(1) - Nominell kylkapacitet baseras på: inomhustemp.: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","","(2) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]
["","","","","","(3) - Se separat ritning för driftsområde"]
["","","","","","(4) - Se separata ritningar för elektriska data"]