{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ71C8VEB / RZQSG71L3V1B","FBQ100C8VEB / RZQSG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L9V1B","FBQ125C8VEB / RZQSG125L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L9V1B"]
["Kylkapacitet","Nom.","","kW","6.8","9.5","","12.0"]
["Rumskyla","SEER","","","5.81","5.50","5.10","5.20","4.80"]
["","Årlig energiförbrukning","","kWh/a","410","605","652","808","875"]
["","Kapacitet","Pdesign","kW","6.80","9.50","9.50","12.00","12.00"]
["","Energieffektivitetsklass","","","A+","A","B","A","B"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.00","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.88","4.01","3.80","3.90","3.80"]
["","Energieffektivitetsklass","","","A","A+","A","A","A"]
["","Årlig energiförbrukning","","kWh/a","2,166","2,654","2,800","2,729","2,800"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","1,035","1,435","","1,870"]
["","EER köldfaktor","","","3.28","3.31","","3.21"]
["","COP","","","3.61","3.65","","3.51"]
["","Energimärkningsdirektiv","Kyla","","A","A","","A"]
["","","Värme","","A","A","","B"]
["Uppvärmningseffekt","Nom.","","kW","7.5","10.8","","13.5"]
["Anm:","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]
["","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]