{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":23,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ100D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ100D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG125L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG125L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG125L9V1B","FBQ140D2VEB / RZQG140L9V1B","FBQ71D2VEB / RZQG71L9V1B (Archived)","FBQ60D2VEB / FBQ60D2VEB / RZQG125L9V1B (Archived)","FBQ125D2VEB / RZQG125L9V1B (Archived)"]
["Kylkapacitet","Nom.","","kW","","","","","","9.5 (2)","","","","","","","","","","13.4 (2)"]
["Rumskyla","SEER","","","6.16","5.10","5.10","5.10","5.10","5.87","5.87","5.10","5.10","5.10","5.10","6.11","5.10","5.10","5.10"]
["","Årlig energiförbrukning","","kWh/a","386","466","466","466","652","566","566","652","652","652","652","687","824","824","824"]
["","Kapacitet","Pdesign","kW","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energieffektivitetsklass","","","A++","A","A","A","A","A+","A+","A","A","A","A","A++","A","A","A"]
["Rumsvärme (medelklimat)","Kapacitet","Pdesign","kW","6.00","6.00","6.00","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.70","12.71","12.71","12.71"]
["","SCOP/A","","","4.31","3.80","3.80","3.80","3.80","4.78","4.78","3.80","3.80","3.80","3.80","4.28","3.80","3.80","3.80"]
["","Energieffektivitetsklass","","","A+","A","A","A","A","A++","A++","A","A","A","A","A+","A","A","A"]
["","Årlig energiförbrukning","","kWh/a","1,949","2,210","2,210","2,210","4,163","3,310","3,310","4,163","4,163","4,163","4,163","4,154","4,683","4,683","4,683"]
["Nominell verkningsgrad","Årlig energiförbrukning","","kWh","","","","","","1,247"]
["","EER köldfaktor","","","","","","","","3.81 (1)","","","","","","","","","","3.35 (1)"]
["","COP","","","","","","","","4.41 (1)","","","","","","","","","","3.60 (1)"]
["","Energimärkningsdirektiv","Kyla","","","","","","","A"]
["","","Värme","","","","","","","A"]
["Uppvärmningseffekt","Nom.","","kW","","","","","","10.80 (2)","","","","","","","","","","15.50 (2)"]
["Anm:","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","","","","","","","","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU","","(1) - EER/COP enligt Eurovent 2012, endast för användning utanför EU"]
["","","","","","","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","","","","","","","","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last","","(2) - Nominell verkningsgrad: kyla vid 35°/27° nominell last, värme vid 7°/20° nominell last"]
["Utomhusdel","","","","","","","","","","","","","","","","","","","","RZQG71L9V1","RZQG125L9V1","RZQG125L9V1"]
["Kylkapacitet","Nom.","","kW","","","","","","","","","","","","","","","","","6.8","","12.0"]
["Värmekapacitet","Nom.","","kW","","","","","","","","","","","","","","","","","7.5","","13.5"]
["Nominell verkningsgrad","EER köldfaktor","","","","","","","","","","","","","","","","","","","3.53","","3.83"]
["","COP","","","","","","","","","","","","","","","","","","","3.96","","3.83"]
["","Årlig energiförbrukning","","kWh","","","","","","","","","","","","","","","","","963","","1567"]
["","Energimärkningsdirektiv","Kyla","","","","","","","","","","","","","","","","","","A","","A"]
["","","Värme","","","","","","","","","","","","","","","","","","A","","A"]
["Rumskyla","Energieffektivitetsklass","","","","","","","","","","","","","","","","","","","A++","A","A+"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","","","","","6.80","12.00","12.00"]
["","SEER","","","","","","","","","","","","","","","","","","","6.16","5.10","5.83"]
["","Årlig energiförbrukning","","kWh/a","","","","","","","","","","","","","","","","","386","824","720"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","","","","","","","","","","","","","","","","","A+","A","A+"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","","","","","6.00","12.71","12.70"]
["","SCOP/A","","","","","","","","","","","","","","","","","","","4.35","3.80","4.37"]
["","Årlig energiförbrukning","","kWh/a","","","","","","","","","","","","","","","","","1931","4683","4069"]