{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RQ-BW1"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / RQ71B8W1B","FCAG100AVEB / RQ100B8W1B","FCAG125AVEB / RQ125B8W1B"]
["Kylkapacitet","Nom.","","kW","7.10 (1)","10.0 (1)","12.5 (1)"]
["Nominell verkningsgrad","EER köldfaktor","","","2.70","2.81","2.69"]
["","Årlig energiförbrukning","","kWh","1,315","1,780","2,325"]
["","COP","","","2.89","3.06","2.89"]
["","Energimärkningsdirektiv","Kyla","","D","C","D"]
["","","Värme","","D","D","D"]
["Uppvärmningseffekt","Nom.","","kW","8.00 (2)","11.2 (2)","14.6 (2)"]
["Anm:","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT; ekvivalent rörledningslängd: 5 m, nivåskillnad: 0 m"]
["","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m"]