{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXM-N9"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / RXM35N2V1B9"]
["Kylkapacitet","Nom.","","kW","3.50"]
["Värmekapacitet","Nom.","","kW","4.20"]
["Nominell verkningsgrad","EER köldfaktor","","","3.72"]
["","COP","","","3.77"]
["","Årlig energiförbrukning","","kWh","471"]
["","Energimärkningsdirektiv","Kyla","","A"]
["","","Värme","","A"]
["Rumskyla","Energieffektivitetsklass","","","A++"]
["","Kapacitet","Pdesign","kW","3.50"]
["","SEER","","","6.35"]
["","Årlig energiförbrukning","","kWh/a","193"]
["Rumsvärme (medelklimat)","Energieffektivitetsklass","","","A++"]
["","Kapacitet","Pdesign","kW","3.32"]
["","SCOP/A","","","4.90"]
["","Årlig energiförbrukning","","kWh/a","948"]
["Anm:","","","","(1) - Se separata ritningar för elektriska data"]
["","","","","(2) - Se separat ritning för driftsområde"]
["","","","","(3) - Nominell kylkapacitet baseras på: inomhustemperatur: 27°CTT, 19°CVT, utomhustemperatur: 35 °CTT, ekvivalent köldmedierörledning: 5 m, nivåskillnad: 0 m."]
["","","","","(4) - Nominella värmekapaciteter baseras på: inomhustemperatur: 20°CTT, utomhustemperatur: 7 °CTT, 6 °CVT, ekvivalent köldmedierörledning: 5m, nivåskillnad: 0 m."]